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Potential unexpected problems, their probable causes and possible solutions. Use this chart in training and keep a copy at the site. Seek technical assistance if a problem cannot be solved with these steps.
	Problem
	Probable cause
	Possible solution

	Wind pump does not self-furl
	• Furling mechanism not working
	• Repair the furling system.

	Windmill working but no water being raised
	• Borehole has run dry
• Pump washers leaking
• Leaky riser
	• Remove the pump and inspect or repair. Use the dipper to check the water level in the borehole.
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